Adaptec 7800 Family Manager Set v3.02.2

README for Microsoft Windows 95

The following information is available in this README file:

Supported Hardware

Changes From Prior Release

Installation Instructions

> - Installing the Driver When Installing Windows 95
> - Updating the Driver for Windows 95 (Retail Edition)
> - Updating the Driver for Windows 95 (OSR2.x)

Known Issues

Diskette Contents

Contacting Adaptec

Supported Hardware

The following Adaptec SCSI Host Adapters are supported by the 7800 FMS v3.02.2. The first list (Fast/Ultra Adapters) is supported by the AIC78xx.MPD driver, while the second list (Ultra2 Adapters) is supported by the AIC78U2.MPD driver.

Fast/Ultra Adapters Description

AVA-2902I | PCI-to-Fast SCSI (non-bootable, internal)
AVA-2902E | PCI-to-Fast SCSI (non-bootable, external)
AVA-2903 | PCI-to-Fast SCSI (non-bootable, internal, external)
AVA-2904 | PCI-to-Fast SCSI (non-bootable)
AVA-2906 | PCI-to-Fast SCSI (non-bootable, internal, external)
AHA-2910C | PCI-to-Fast SCSI (non-bootable)
AHA-2915C | PCI-to-Fast SCSI (non-bootable)
AHA-2920C | PCI-to-Fast SCSI
AHA-2930C | PCI-to-Ultra Single-ended SCSI
AHA-2940 | PCI-to-Fast SCSI
AHA-2940W | PCI-to-Fast and Wide Single-ended SCSI
AHA-2940AU | PCI-to-Ultra Single-ended SCSI
AHA-2940U | PCI-to-Ultra Single-ended SCSI
AHA-2940U Dual | DualChannel PCI-to-Ultra Wide Internal Single-ended SCSI with 50-pin external connector
AHA-2940UW | PCI-to-Ultra Wide Single-ended SCSI
AHA-2940UW Pro | PCI-to-Ultra Wide Single-ended SCSI (See Changes From Prior Release Section)
AHA-2940UW Dual | DualChannel PCI-to-Ultra Wide Single-ended SCSI with 68-pin external connector
AHA-2944W | PCI-to-Fast and Wide Differential SCSI
AHA-2944UW | PCI-to-Ultra Wide Differential SCSI
AHA-3940 | MultiChannel PCI-to-Fast SCSI
AHA-3940W | MultiChannel PCI-to-Fast and Wide SCSI
AHA-3940U | MultiChannel PCI-to-Ultra SCSI
AHA-3940UW | MultiChannel PCI-to-Ultra Wide SCSI
AHA-3940UWD | MultiChannel PCI-to-Ultra Wide SCSI with dual external VHD connectors
AHA-3944UWD | MultiChannel PCI-to-Ultra Wide Differential SCSI with dual external VHD connectors
AHA-3940AU | MultiChannel PCI-to-Ultra SCSI
AHA-3940AUW | MultiChannel PCI-to-Ultra Wide SCSI
AHA-3940AUWD | MultiChannel PCI-to-Ultra Wide SCSI with dual VHD external connectors
AHA-3944AUWD | MultiChannel PCI-to-Ultra Wide Differential SCSI with dual external VHD connectors
AHA-4944W | Quad Channel PCI-to-Fast and Wide Differential SCSI
AHA-4944UW | Quad Channel PCI-to-Ultra Wide Differential SCSI
APA-1480 | CardBus-to-Ultra Single-ended SCSI
AIC-7850 | Single-chip PCI-to-Fast SCSI
AIC-7855 | Single-chip PCI-to-Fast SCSI
AIC-7856 | Single-chip PCI-to-Fast SCSI
AIC-7860 | Single-chip PCI-to-Ultra SCSI
AIC-7870 | Single-chip PCI-to-Fast and Wide SCSI
AIC-7880 | Single-chip PCI-to-Ultra Wide SCSI
AIC-7895 | Single-chip PCI-to-MultiChannel Ultra Wide SCSI

Ultra2 Adapters Description

AHA-2940U2 OEM | PCI-to-Ultra2 Wide LVD/Single-ended SCSI
AHA-2940U2B | PCI-to-Ultra2 Wide LVD SCSI
AHA-2940U2W | PCI-to-Ultra2 Wide LVD/Single-ended SCSI
AHA-2950U2B | 64-bit PCI-to-Ultra2 Wide LVD SCSI
AHA-3950U2B | 64-bit PCI-to-MultiChannel Ultra2 Wide LVD SCSI
AHA-3950U2D | 64-bit PCI-to-MultiChannel Ultra2 Wide LVD SCSI with dual external VHD connectors
AIC-7890 | Single-chip PCI-to-Ultra2 SCSI
AIC-7891 | Single-chip 64-bit PCI-to-Ultra2 SCSI
AIC-7896 | Single-chip PCI-to-MultiChannel Ultra2 SCSI
AIC-7897 | Single-chip 64-bit PCI-to-MultiChannel Ultra2 SCSI

Changes From Prior Release

This release of the Adaptec 7800 Family Manager Set v3.02.2 adds the following support from the previous v3.02 release:

> - Support for the AHA-2940UW Pro

> > 1) Adds the ability to use all three connectors at the same time
> > 2) Current Sensing Circuit checks for improper termination

> - Support for the AHA-3950U2D

> > 1) Adds two external VHD connectors instead of one wide external connector

Installation Instructions

If you are performing a first time Windows 95 installation, see the "Installing the Driver When Installing Windows 95" section, below. If Windows 95 is already installed on your system, see the "Updating the Driver for Windows 95" section.

NOTE: Windows 95 shipped in two different version - the Retail Edition and the OEM Service Release 2 (or OSR2) Edition. Both versions function the same, but the process of installing drivers is different. To determine which version you have, follow these steps:

1. Select Control Panel under Settings from the Start Menu.
2. Double-click the "System" icon.
3. Under the "General" tab, it will display the version number of Windows 95 under the System category.
4. If it displays "4.00.950", you have the Retail Edition installed. If it displays "4.00.950 B", you have OSR2 installed.

Installing the Driver When Installing Windows 95

A fresh Windows 95 installation will attempt to detect all Adaptec SCSI host adapters in your system. If it is unable to do so, follow the instructions in the "Updating the Driver for Windows 95" section below.

NOTE: When Windows 95 starts, if "New Hardware Found" is displayed, select "Driver from disk provided by hardware manufacturer". Insert your Adaptec 7800 Family Manager Set v3.02.2 Diskette and type a:\win9x as the path; follow the on-screen instructions.

Updating the Driver for Windows 95 (Retail Edition)

To update or install the aic78xx.mpd or aic78u2.mpd driver if Windows 95 is already installed, follow these instructions:

1. Start Windows 95.

2. Click the Start button on the Windows 95 task bar, and then point to Settings.

3. Click Control Panel.

4. Double-click the System icon.

5. On the Device Manager tab, click the plus sign next to the SCSI controller icon.

NOTE: If Windows 95 cannot determine the type of host adapter installed in your computer, a yellow question mark labeled Other devices appears instead of the SCSI controller icon. To continue, click the plus sign next to the question mark; a yellow question mark labeled PCI SCSI Bus Controller then appears.

6. Double-click the 7800 Family host adapter you wish to update, or if a yellow question mark labeled PCI SCSI Bus Controller is displayed, double-click the question mark.

7. Insert the Adaptec 7800 Family Manager Set v3.02.2 Diskette into drive A:.

8. Select the Driver tab.

NOTE: If the version of Windows 95 you are using now displays a window with a Update Driver button instead of a Change Driver button, the remainder of your install procedure is covered in Updating the Driver for Windows 95, Version OSR 2, described below.

9. Click Change Driver. You may be asked to select the hardware type; if so, select SCSI Controllers.

10. Click the Have Disk button and enter a:\win9x as the path.

11. Click OK.

12. Select the Adaptec 7800 Family host adapter, and click OK.

13. Again, click OK. The driver is now installed.

14. You must restart your computer for the changes to take effect. Click Yes to restart your computer. Click No to return to the system properties window.

Updating the Driver for Windows 95 (OSR2.x)

This section covers the remaining steps to updating the driver on Windows 95 OSR2.

NOTE: If you have not already done so, follow the instructions in "Updating the Driver for Windows 95" section above.

1. Click Update Driver.

2. Insert the Adaptec 7800 Family Manager Set v3.02.2 diskette into drive A:.

3. In the Update Device Driver Wizard, select Yes, and click Next.

4. Select Other locations.

5. Under the Location edit box, type a:\win9x, then click OK.

6. Click the Finish button.

7. At the message "Please insert the disk labeled '7800 Family Manager Set v3.02.2 Installation Disk'." Insert the Adaptec 7800 Family Manager Set v3.02.2 diskette and click OK.

8. Another dialog box, Copying Files, appears with the message "The file 'AIC78XX.MPD' or 'AIC78U2.MPD' on 7800 Family Manager Set v3.02.2 Installation Disk could not be found ...". Type a:\win9x in the Copy Files from the edit box and click OK. The driver is now installed.

9. You must restart your computer for the changes to take effect. Click Yes to restart your computer. Click No to return to the system properties window.

NOTE: If you attempt to re-update the driver again, at step 3 above you will need to select No, click Next, and follow the on-screen instructions to re-update.

Known Issues

- In some cases, each channel of a MultiChannel adapter must be updated/installed manually with the aic78xx.mpd driver on a freshly installed Windows 95 system. Please follow the instructions listed under "Updating the Driver for Windows 95" for each channel.

- Real mode ASPI drivers from EZ-SCSI are not needed, because Windows 95 miniport drivers support most SCSI host adapters and SCSI devices. However, you will need to load the ASPI drivers (including MSCDEX.EXE, if you have CD-ROM drive) if any of the following are true:

- You are running in MS-DOS mode and need to access your CD-ROMdrive.
- You are using a scanner or another SCSI device with CONFIG.SYS or AUTOEXEC.BAT based drivers, such as HP's SJIIX.SYS.
- You have an older model SCSI-1 CD-ROM driver that Windows 95 does not support.
- You are using a CD-Recorder drive (however, some newer models of CD-Recorder drives can use the embedded Windows drivers).

- Some older models of SCSI CD-ROM drives are not compatible with the embedded Windows 95 CD-ROM driver. You can add support for the CD-ROM drive by doing the following:

- Make sure your ASPI real mode drivers (including ASPI8DOS.SYS, ASPICD.SYS and MSCDEX.EXE) are loaded and running from your CONFIG.SYS and AUTOEXEC.BAT files. Consult your EZ-SCSI installation guide for more details.
- If step 1 did not work, find the file named CDTSD.VXD in the \windows\system\iosubsys directory and rename it to CDTSD.SAV.

- The mapping between MSCDEX.EXE, which runs in real mode, and theWindows 95 CD-ROM driver does not match. You can correct this in one of two ways:

- Comment out the line that loads mscdex.exe in the autoexec.bat file.
- Change the /L switch on the line that loads mscdex.exe in the AUTOEXEC.BAT file so it assigns the CD-ROM drive the next highest logical drive letter after the hard disk drives.

- Windows 95 does not support sharing of system interrupts (also known as IRQs) between two or more I/O subsystem devices (i.e. network interface cards or hard disk adapters such as SCSI host adapters). When IRQs are shared between I/O devices, lockups can occur while booting. If lockups occur, try moving or removing one or more PCI cards from one slot to another and bootup your computer again. If problems continue, refer to your system documentation and/or your system technical support for information on adding your system configuration.

- When updating/installing the driver for a host adapter, the Family Manager Set v3.02.2 will not automatically install both Ultra2 and Ultra/Fast drivers. If you require both drivers, you will have to install them seperately, as per individual host adapter. For example, after installing the driver for the AHA-2940U2W, there may be a conflict in the Device Manager with an existing or newly-installed Adaptec UltraSCSI or earlier host adapter. To resolve this problem, simply update the driver for the conflicting host adapter with the Family Manager Set v3.02.2 driver from the Device Manager.

Diskette Contents

The following files are included in this diskette:

\WIN9X\AIC78XX.MPD | 7800 series SCSI miniport for Windows 95/98
\WIN9X\AIC78U2.MPD | 7800 series Ultra2 SCSI miniport for Windows 95/98
\WIN9X\AIC78XX.INF | Install script used by Windows 95/98 setup
\WIN9X\README95.TXT | Readme file for Windows 95
\WIN9X\README98.TXT | Readme file for Windows 98
\WIN9X\README95.HTM | HTML version of README95.TXT (this file)
\WIN9X\README98.HTM | HTML version of README98.TXT
\WIN9X\ADPINSTR.VXD | Instrumentation Helper Virtual Device Driver

Contacting Adaptec

Electronic Support

Technical information, including product literature, answers to commonly asked questions, information on software upgrades and other topics is available electronically through the following:

- Adaptec World Wide Web (WWW) site at http://www.adaptec.com.
- File Transfer Protocol (FTP) server at ftp://ftp.adaptec.com.
- To submit your electronic mail message to Adaptec Technical Support use the product support information Webmail form at: http://www.adaptec.com/support/webmail.html.
- Adaptec USA Bulletin Board Service (BBS) at 408-945-7727; supports up to 28,800 bps (bits per second), 8 data bits, 1 stop bit, no parity. No product literature is available on the Adaptec BBS.
- Interactive Fax System at 303-684-3400; available 23 hours a day, 7 days a week. The fax system is out of service 1 hour each day.

Technical and Product Support

- To speak with a product support representative, call 408-934-SCSI (7274), M-F, 6:00 a.m. to 5:00 p.m., Pacific Time. After hours, on weekends, and on holidays, product support is also available for a fee at 800-416-8066.
- For electronic technical support and information about many of Adaptec's other electronic support services, or to use the Adaptec Interactive Support System call 800-959-SCSI (7274) or 408-945-2550, 24 hours a day, 7 days a week. The system prompts you with questions regarding your problem and then provides step-by-step troubleshooting instructions.

Sales and Ordering Information

- For sales information, call 800-442-SCSI (7274), M-F, 6:00 a.m. to 5:00 p.m., Pacific Time, or 408-945-8600 and ask for Inside Sales, M-F, 8:00 a.m. to 5:00 p.m., Pacific Time.
- To order Adaptec software and SCSI cables, call 800-442-SCSI (7274), M-F, 6:00 a.m. to 5:00 p.m., Pacific Time.
- To request additional documentation for Adaptec products, call 800-934-2766 or 510-732-3829, M-F, 6:00 a.m. to 5:00 p.m., Pacific Time.