Readme for Sirona Reconstruction Server, Version 2.2

# Information on the Sirona Reconstruction Server CD

This CD contains the Sirona Reconstruction Server in German and in other language versions as required. The relevant version number is displayed during setup.

Current publication number of Installation Manual: D3437.031.02.06.02

## Notes

- In the case of standalone systems (laptops), it is important to ensure that the MS Loop Back Adapter is installed.

## Components of the Sirona Reconstruction Server

- Sirona Control Server: Acquisition of exposures and management of license information
- Sirona Reconstruction Server: Reconstruction of 3D volumes

All components require SIDEXIS XG V 2.4 or higher. Therefore SIDEXIS must be installed before the Sirona Reconstruction Server, as described in the SIDEXIS manual.

## What do you have to do following the installation?

- The devices are configured using the "Configuration of X-ray components" application (SiXABCon). This is started via the SIDEXIS Manager.

# Installing the Sirona Reconstruction Server

The CD usually starts automatically after it is inserted in the drive. If this is not the case, start the setup routine manually by executing the "autorun.exe" file in the root directory of the CD.

The rest of the installation is menu-driven. During the installation procedure, the required information is queried. This ensures that the correct configuration is performed automatically.

# Requirements for installing/operating a Sirona Reconstruction Server

Operating system:

- Windows XP Professional Workstation (Service Pack 3 or newer)
- Windows 7 Ultimate, 64-bit

| Minimum requirements | Recommended configuration
Processor | Dual core, 2GHz or higher | Quad core, 2GHz or higher
Main memory | 4GB RAM | 4GB RAM
Hard disk | Min. 500 GB free memory | Min. 1 TB free memory
Exchangeable media | DVD-ROM (dual-layer) | DVD-ROM (dual-layer)
Operating system | Windows XP Professional (32-bit) SP3 Windows 7 Professional (32- or 64-bit) | Windows 7 Ultimate, 64-bit
Graphics card | external, > 512MB, minimum resolution 1280*1024, 16.7 mil. colors (TrueColor), Shader Model 3 for advanced rendering in GALILEOS Implant | external, > 512MB, minimum resolution 1280*1024, 16.7 mil. colors (TrueColor), Shader Model 3 for advanced rendering in GALILEOS Implant
Monitor | suitable for diagnostic applications | suitable for diagnostic applications
Network interface card | Network RJ45, 100 MBit/s | Network RJ45, 1 GBit/s

The installation requires the user to log in as an administrator. To install the Sirona Reconstruction Server components, you will need read/write/change/execute access rights for the \SIDEXIS, \PDATA and \Programs\Sirona directories. These are automatically set during installation.

# New features of the Sirona Reconstruction Server 2.2 - Overview

- Calibration improved

# Changelog - History

## Sirona Reconstruction Server 2.1 Changes

- MARS: Metall artifact reduction (ORTHOPHOS XG 3D)
- HD Mode: High Definition mode (ORTHOPHOS XG 3D)
- Image quality improvement: Homogenity (GALILEOS and ORTHOPHOS XG 3D)
- Image quality improvement: Contrast (GALILEOS and ORTHOPHOS XG 3D)

## Sirona Reconstruction Server 2.0 Changes

- Metal artefact reduction

## Sirona Reconstruction Server 1.8 Changes

- Support for ORTHOPHOS XG 3D

## Sirona Reconstruction Server 1.7.2 Changes

- The tolerance lines for the thyroid protection border have been removed from the service exposure for collimation adjustment.
- Dosage display in Sidexis: The dosage is now displayed in the "Write image" dialog.
- Improved reconstruction: Improved homogeneity in the volume (soft tissue and bones) and improved view outside the 100% volume.
- Third-party export supports resolutions of 0.15mm and 0.2mm and 16 Bit export.

## Sirona Reconstruction Server 1.7 Changes

- All components support auto-update via XGNetDeploy
- New languages: Chinese Simplified, Chinese Traditional
- Changes to allow GALILEOS mechanical blind
- Sirona Control Admin includes detailed information on license use
- Additional (Asian) character sets available on GALILEOS display
- Classic PAN artefact reduction
- Classic PAN function available with all systems
- Calibration improved in user interface and result
- Reconstruction algorithm changed to improve SNR and homogeneity within the volume
- Sirona Control Server includes a restart button for a hard RCU boot
- Windows Vista support for GALILEOS Server

## Sirona Reconstruction Server 1.6 Changes

- Adjustments for GALILEOS Comfort to account for new license IDs
- Classic-PAN: New panorama image with typical OPG blurring (depending on licensing and regional regulatory approval)

## Sirona Reconstruction Server 1.5 Changes

- Integrated function creates GALILEOSViewer CD including patient scan.
- Faster data reconstruction
- Faster data transfer from GALILEOS to RCU due to data compression
- Additional languages: Japanese, Korean, Dutch, Portuguese, Russian
- One Button Rescue
- Empty DataContainers are deleted at service start.
- New standard scan "Volume2" creates raw volume with 3ooµm resolution, allowing faster data processing with smaller file size.
- Reduction of data size: Reconstructed volumes are 180 instead of 256 MB.

## Sirona Reconstruction Server 1.4 Changes

- Sirona Control Server can be launched from any workstation
- For rescue cases or license administration, Sirona Control Admin can be launched easily from Sidexis Manager
- Dosage measurement changed to constant radiation in order to increase the number of available dosage measuring devices.

# Hotline

In case you have any questions or need assistance with a particular problem:
Phone +49 (0) 62 51 / 16 - 16 16

Contact form for technical requests

Enjoy working with the Sirona Reconstruction Server and thank you for placing your confidence in our products.

Your SIDEXIS Team

Sirona Dental Systems GmbH
Fabrikstr. 31
64625 Bensheim, Germany