[Menu]
1=X-RAY SENSOR
2=Start when Windows® starts
3=Configuration
4=Remaining images
5=Exit
10=Display new image during 
11=No display
12=sec
13=Permanently
14=Enable connection
15=Disable connection at timeout
20=Display sensor orientation during
21=Update firmware now



[Strings]
100=Activate/Deactivate Sensor
101=Checked: Connected mode/Unchecked: Disconnected mode
301=Not checked: Standard Resolution- Faster acquiry- More sensible to x-ray radiation
302=Checked: Full Resolution- Produce a full resolution image- Show more detailed diagnostic informations
500=Warning: You are about to change your WI-FI parameters. Read carefully the user manual before doing this command.
501=Your action has been taken in account.
1000=A NEW FIRMWARE UPDATE IS AVAILABLE. Right click on the bar or the icon to start the update.


[Config]
0=CONFIGURATION
1=OK
2=Cancel
160=Model
128=PCI
129=USB
163=Tool bar
132=Visible
130=Full resolution
133=With extension
161=Behavior
127=Show activation button
101=Activate during:
102=minutes
125=Permanently
162=Image processing
118=Equalize
116=Sharpen
328=Date and time on image
330=Factory Settings
331=Text Size
332=Expo params on image

456=Film alike
457=Auto contrast
458=Test mode



;229=USB
;228=PCI
;230=Krystal-X Wifi
;236=DSX730 V1 - 100
;237=DSX730 V2 - 100
;238=DSX730 V3 Evo1 & 2 - 103
;239=DSX730 V3 - 104
;240=Upix - 102
;241=DSX730 Evo3 - 501
;242=Krystal-X - 500




[LastImages]
0=REMAINING IMAGES
1=Load
2=Cancel
10=Please confirm
11=Warning
1016=Preview
1018=Delete
1017=Delete on load

[WIFIX]
1=Write
2=Cancel
450=IP Address 
451=Sub-Net Mask
452=Channel
453=SSID
454=Read current
455=Default

