Display driver

Location of the Display driver installer:

- x:\Drivers\Disp_driver (The letter ‘x’ means the drive letter of the CD-rom).

Installation

Follow instructions below.

1. Start SmartPad PC and login to the Windows®

2. Close SmartNav program if it runs

3. If “Welcome to the Found New Hardware Wizard” dialog opens then close it.

4. Place SmartNav installation CD to the CD-rom drive (if SmartNav installation window opens then click exit)

5. Open Windows® explorer and browse to the x:\Drivers\Disp_driver folder

6. Double click Setup.exe icon to start the driver installer

7. Click “NEXT”

8. Click “YES” and wait a moment until installation is completed

9. Click “FINISH” to re-start SmartPad PC

Un-installation

Follow instructions below.

1. Start SmartPad PC and login to the Windows®

2. Close SmartNav program if it runs

3. Select “START => CONTROL PANEL => PERFORMANCE AND MAINTENANCE => SYSTEM”.

4. Then select “HARDWARE tab and click “DEVICE MANAGER” button from the device manager.

5. Browse “Display Adapters” and expand it by selecting a “+” symbol on the left hand side of it

6. There are two graphic controllers under “Display Adapter”. Right click first one of the “Intel® 82852/82855...” graphic drivers and select “Un-install”.

7. Click “OK”

8. Click “YES”

9. Re-start SmartPad PC

10. Perform steps from 1 to 5

11. Right click remaining graphic driver under “display adapters” and select “Un-install”

12. Click “OK”

13. Click “YES”

14. Re-start SmartPad PC

Reinstallation

Updating the Display driver requires the un-installation of exist driver first and then new installation is allowed. Follow the Un-installation and Installation sections above to do that.