; dillp.Inf - install information file
; Copyright © 2003 Planmeca Group

[Version]
Signature = "$Chicago$"
ClassGUID = {5BC4C441-DA92-11d5-A7D2-00104B488FAF}
Class = Planmeca
Provider = %PLANMECA%


[Manufacturer]
%PLANMECA% = DeviceList

[DeviceList]
"Planmeca PCI card for Dimax1" = dillp.Install,PCI\VEN_10E8&DEV_1380&SUBSYS_00000000

[DestinationDirs]
dillp.Files.Driver = 10,System32\Drivers
dillp.Files.Driver.NTx86 = 10,System32\Drivers

[SourceDisksNames]
1 = "Planmeca driver disk",,,

[SourceDisksFiles]
dillp.sys = 10,System32\Drivers

[SourceDisksFiles.x86]
dillp.sys = 10,System32\Drivers

;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
; PCI BRIDGE driver
;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
; Windows 98

[Bridge.Install]
CopyFiles = Bridge.Files.Driver
AddReg = Bridge.AddReg

[Bridge.AddReg]
;HKR,,DevLoader,,*ntkern
;HKR,,NTMPDriver,,Bridge.sys

[Bridge.Files.Driver]
;Bridge.sys

;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
; Windows 2000

[Bridge.Install.NTx86]
CopyFiles = Bridge.Files.Driver.NTx86

[Bridge.Files.Driver.NTx86]
;Bridge.sys,,,%COPYFLG_NOSKIP%

[Bridge.Install.NTx86.Services]
AddService = ,%SPSVCINST_ASSOCSERVICE%,


;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
; PCI DRIVER
;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
; Windows 98

[dillp.Install]
CopyFiles = dillp.Files.Driver
AddReg = dillp.AddReg

[dillp.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,dillp.sys

[dillp.Files.Driver]
;dillp.sys

;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
; Windows 2000

[dillp.Install.NTx86]
CopyFiles = dillp.Files.Driver.NTx86

[dillp.Files.Driver.NTx86]
;dillp.sys,,,%COPYFLG_NOSKIP%

[dillp.Install.NTx86.Services]
AddService = Dillp_nt, %SPSVCINST_ASSOCSERVICE%, dillp.Service

[dillp.Service]
DisplayName    = %dillp.ServiceName%
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_DEMAND_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %10%\System32\Drivers\dillp.sys

;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
; Strings

[Strings]
Planmeca = "Planmeca Group"
dillp.ServiceName = "Planmeca DIMAX1 PCI Interface"

SPSVCINST_ASSOCSERVICE=0x00000002	; Driver service is associated with device being installed
COPYFLG_NOSKIP=2			; Do not allow user to skip file
SERVICE_KERNEL_DRIVER=1
SERVICE_AUTO_START=2
SERVICE_DEMAND_START=3
SERVICE_ERROR_NORMAL=1
